For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector at the solenoid valve (1).
2. Disconnect the vacuum hose harness (3).
3. Remove the Nut and solenoid valve (1) from the intake manifold (4).

### Installation Procedure

1. Install the solenoid valve (1) and bracket to the intake manifold (4).

Tighten
Tighten the Nut to 34 N·m (25 lb ft).

2. Connect the vacuum hose harness (3).
3. Connect the electrical connector to the solenoid valve (1).