For 1990-2009 cars

### Removal Procedure

1. Open the window panel.
2. Remove the rear compartment trim as needed. Refer to Liftgate Trim Panel Replacement .
3. Disconnect the rear compartment lid release switch electrical connector. Refer to Rear Compartment Lid Switch Replacement .
4. Disconnect the rear compartment lid lock release actuator secondary lock retainer and electrical connector. Refer to Liftgate Lock Actuator Replacement .
5. Remove the endgate latch bolts (1).
6. Remove the latch (2).

### Installation Procedure

1. Install the latch (2).

Align the holes in the latch with the holes in support.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the endgate latch bolts (1).

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Connect the rear compartment lid lock release actuator electrical connector and secondary lock retainer. Refer to Liftgate Lock Actuator Replacement .
4. Install the rear compartment trim. Refer to Liftgate Trim Panel Replacement .