For 1990-2009 cars

1. Spray the ends of the transmission oil pan screws with penetration oil.
2. Remove the transmission oil pan screws.
3. Remove the transmission oil pan and the transmission oil pan gasket.
4. Remove the transmission oil filter assembly.

4.1. | Pry the metal from the top of the filter and pull the top away.

4.2. | Open the filter.

5. The filter may need diagnosis. Inspect the following items for wear or corrosion:

• | Clutch material

• | Bronze slivers indicating bushing wear

• | Steel particles

6. Remove the oil filter seal.