For 1990-2009 cars

### Inspection Procedure

1. Inspect the spark plug gap. Adjust as needed.
2. Inspect the spark plug wires for any obvious cuts, burns, or damage. replace as needed.
3. With the engine ON, inspect for any arcing to ground or other components. Replace the wires as required.
4. Connect an ohmmeter to the end of each suspect wire. If the meter reads over 30,000 ohms, replace the wire.