For 1990-2009 cars

The cooling fan relays are used to control the high current flow to power the cooling fan motors. Both fans operate together. When minimum cooling is required, the PCM energizes cooling fan relay #1 and both fans operate at low speed, since the fans are connected in series through cooling fan relay #2 and #3. When maximum cooling is required, the PCM energizes all three cooling fan relays. The left fan is still powered through cooling fan relay #1, but is now grounded through cooling fan relay #3. The right fan is now powered directly through cooling fan relay #2 and both fans operate at high speed.