For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire Power Folding Top System Check performed? | -- | Go to Step 2 | Go to Power Folding Top System Check
2 |

1. Turn the ignition switch to the RUN position.
2. Use a test light in order to backprobe between folding top switch connector terminal F and ground.

Does the test light illuminate?

--

Go to Step 3

Go to Step 4

3 |

1. Use a test light in order to backprobe between folding top switch connector terminal A and ground.
2. While observing the test light, press the folding top switch to the DOWN position.

Does the test light illuminate?

--

Go to Step 5

Go to Step 6

4 | Repair the open in circuit 341, between the folding top switch terminal F and the IP fuse block. Is the repair complete? | -- | Go to Step 13 | --
5 | Use a test light in order to backprobe between folding top switch connector terminal E and B+. Does the test light illuminate? | -- | Go to Step 8 | Go to Step 7
6 |

1. Test for a poor connection at the folding top switch connector terminal A and terminal F.
2. If the connection is OK, replace the folding top switch.

Is the repair complete?

--

Go to Step 13

--

7 | Use a test light in order to backprobe between folding top switch connector terminal H and B+. Does the test light illuminate? | -- | Go to Step 14 | Go to Step 15
8 |

1. Disconnect the folding top pump assembly connector.
2. Connect a test light between folding top pump assembly connector terminal B (the instrument panel harness side) and ground.
3. While observing the test light, press the folding top switch to the DOWN position.

Does the test light illuminate?

--

Go to Step 10

Go to Step 9

9 | Repair an open or a short to ground in circuit 163, between the folding top switch and the convertible folding top pump assembly. Is the repair complete? | -- | Go to Step 13 | --
10 |

1. Connect a test lamp between top pump assembly connector terminal A (on the instrument panel harness side) and ground.
2. While observing the test light, press the folding top switch to the UP position.

Does the test light illuminate?

--

Go to Step 12

Go to Step 11

11 | Repair an open or a short to the ground in circuit 162, between the folding top switch and the folding top pump assembly. Is the repair complete? | -- | Go to Step 13 | --
12 |

1. Test for a poor connection at the folding top pump assembly.
2. If the connection is OK, replace the folding top pump assembly. Refer to Power Folding Top Pump with Motor Replacement .

Is the repair complete?

--

Go to Step 13

--

13 |

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors/components removed.

Have all the repairs been made?

--

Go to Power Folding Top System Check

--

14 |

1. Test for a poor connection at folding top switch connector terminal E.
2. If the connection is OK, replace the folding top switch.

Is the repair complete?

--

Go to Step 13

--

15 | Repair the poor connection or open in circuit 1350. Is the repair complete? | -- | Go to Step 13 | --