For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire Exterior Lights System Check performed? | -- | Go to Step 2 | Go to Exterior Lights System Check
2 |

1. Turn the ignition switch to the OFF position.
2. Place the turn signal in the OFF position.
3. Disconnect the turn signal switch C216.

Are the turn signal lamps on?

--

Go to Step 3

Go to Step 4

3 |

• | The LH turn signal is on at all times: Repair a short to B+ on CKT 18.

• | The RH turn signal is on at all times: Repair a short to B+ on CKT 19.

Is the repair complete?

--

Go to Step 5

--

4 | Replace the turn/hazard switch assembly. Refer to Hazard Warning Switch Replacement . Is the repair complete? | -- | Go to Step 5 | --
5 |

1. Turn the ignition switch to the OFF position.
2. Reconnect all of the connectors and components that were previously removed.

Have all repairs been made?

--

Go to Exterior Lights System Check

--