For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 36660-A Torque Angle Meter

J 37096 Flywheel Holding Tool

1. Remove the transmission. Refer to SECTION 7A or SECTION 7B.
2. For manual transmission, remove the flywheel housing. Refer to SECTION 7B.
3. Remove the flywheel bolts.
4. Remove the flywheel. Use the J 37096 in order to prevent crankshaft rotation.

### Installation Procedure

1. Install the flywheel. Use the J 37096 in order to prevent the crankshaft from rotating.
2. Install the flywheel bolts.

Tighten
Tighten the flywheel bolts to 15 N·m (11 lb ft). Use the J 36660-A in order to rotate the bolts an additional 50 degrees.

3. For manual transmission, install the flywheel housing. Refer to SECTION 7B.
4. Install the transmission. Refer to SECTION 7A or SECTION 7B.