For 1990-2009 cars

# FRT. INBOARD BRAKE SHOE RATTLE NEW ANTI-RATTLE SPRING

SOME 1982 CAMAROS AND "S" TRUCKS MAY EXHIBIT A FRONT INBOARD BRAKE SHOE RATTLE. A NEW ANTI-RATTLE SPRING HAS BEEN RELEASED FOR PRODUCTION AND USAGE IMPLEMENTED AT THE SOURCE ON JULY 5, 1982. VEHICLES EXHIBITING THIS CONDITION CAN BE CORRECTED BY REPLACING THE EXISTING ANTI-RATTLE SPRINGS WITH NEW SPRINGS CONTAINED IN KIT, P/N 18006810, AVAILABLE FROM WDDGM. USE APPLICABLE LABOR OPERATION.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.