For 1990-2009 cars

## Exhaust Tail Pipe Extension Chevrolet / Pontiac

### Removal Procedure

1. Loosen the exhaust tail pipe extension clamp bolt/screw.
2. Remove the exhaust tail pipe extension from the exhaust muffler tail pipe.

### Installation Procedure

1. Push the exhaust muffler tail pipe extension on to the exhaust muffler tail pipe until the stop position is reached.

Important: The WS6 (Pontiac Only) exhaust tail pipe extension to rear fascia alignment specifications, depending on the model, are the same as either the Pontiac Formula coupe, or Pontiac Trans Am coupe.

2. Align the exhaust tail pipe extension to the rear fascia.
3. Tighten the exhaust tail pipe extension clamp.

Tighten
Tighten the extension clamp bolt to 68 N·m (50 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

## Exhaust Tail Pipe Extension Pont w/ Sport Appearance Pkg

### Removal Procedure

1. Loosen the exhaust tail pipe extension clamp nuts.
2. Remove the tailpipe extension from the muffler tailpipe.

### Installation Procedure

Important: If replacement of the exhaust muffler is required, and the vehicle is equipped with the Sport Appearance Package the factory exhaust muffler extensions need to be cut off. Measure 343 mm (13.5 in) from the bend out of the muffler make the cut.

1. Connect the tailpipe extension to the muffler tailpipe.
2. Align the tailpipe extension to the rear fascia.
3. Tighten the exhaust tailpipe extension clamp nuts.

Tighten
Tighten the tailpipe extension clamp nuts to 68 N·m (50 lb ft).