For 1990-2009 cars

### Disassembly Procedure

1. Remove the lock housing cover and sleeve assembly. Refer to Lock Housing Assembly - Disassemble - Off Vehicle .
2. Remove the switch actuator pivot pin (2) from the pivot and pulse switch assembly (1).
3. If removal of the pivot and pulse switch assembly (1) is not needed let the pivot and pulse switch assembly (1) hang freely.
4. Remove the pivot and pulse switch assembly (1) from the lock housing cover and sleeve assembly following these steps:

4.1. | Remove the wire protector shield.

4.2. | Remove the pivot and pulse switch assembly connector from the bulk head connector.

4.3. | Pull the wire harness through the steering column.

| Important: Use care not to damage the wires when pulling the pivot and pulse switch assembly wire harness through the steering column.