For 1990-2009 cars

# SMU - SEC. 5 - REV. FRONT BRAKE ROTOR SPECS.

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 5 - REVISED FRONT BRAKE ROTOR SPECIFICATIONS

#### MODELS: 1995-97 CHEVROLET CAMARO 1995-97 PONTIAC FIREBIRD

THIS BULLETIN IS BEING ISSUED TO REVISE THE FRONT BRAKE ROTOR SPECIFICATIONS IN SECTION 5 OF THE 1995-97 MODEL YEAR SERVICE MANUALS.

THE FOLLOWING ARE THE UPDATED SPECIFICATIONS:

ROTOR THICKNESS (NEW) - 32.0 MM (1.260 IN) MINIMUM ROTOR THICKNESS AFTER REFINISH - 31.08 MM (1.224 IN) DISCARD THICKNESS - 30.70 MM (1.209 IN)

FIGURES: 00

ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1998 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.