For 1990-2009 cars

#### Tools Required

J-25025-5 Guide Pins

1. Install the checkballs (2-6, 8, 12) in the valve body and retain checkballs with Transjel® J 36850 or an equivalent.
2. Install the valve body over the J-25025-5, and connect the manual valve link to the manual valve.
3. Install two bolts to hold the valve body in place.
4. Remove the J-25025-5.
5. Install the fluid level indicator stop bracket (93) and the valve body bolts (62) that are shown only.
6. Finger tighten the bolts.
7. Inspect the Transmission Fluid Pressure Manual Valve Position Switch (TFP Val. Position Sw.) Assembly for the following conditions:

• | Damage

• | Debris

• | Damaged or missing O-rings

• | Cracked connector

• | Loose pins

8. Install the TFP Val. Position Sw. (69) and bolts (62, 70).
9. Inspect the wiring harness solenoid assembly for the following conditions:

• | Damage

• | Cracked connectors

• | Exposed wires

• | Loose pins

10. Install the transmission wiring harness on the valve body.
11. Install the TCC solenoid and bolts (68).

Important: You must tighten certain bolts in a spiral pattern as indicated by the arrows. If you tighten these bolts at random you may distort valve bores. This will inhibit valve operation.

12. Tighten the bolts in the order shown.

Tighten
Tighten the bolts to 11 N·m (8 lb ft).

Refer to Fastener Notice .

Each bolt number refers to a specific bolt size, as indicated by the following list:

• | 1 -- M6 x 1.0 x 65.0

• | 2 -- M6 x 1.0 x 54.4

• | 3 -- M6 x 1.0 x 47.5

• | 4 -- M6 x 1.0 x 35.0

• | 5 -- M8 x 1.25 x 20.0

• | 6 -- M6 x 1.0 x 12.0

• | 7 -- M6 x 1.0 x 18.0

13. Install the TCC PWM solenoid (396) and the solenoid retainer (379).