For 1990-2009 cars

# LTG REQUEST FOR REVIEW UPDATES JULY THRU OCT. 1989

This bulletin addresses changes to the published Pontiac passenger cars Labor Time Guide for July through December, 1989. These changes are the result of dealer "Requests For Review" being handled by C-P-C Technical Service Activity.

These updates will be included in future revisions as printed, and at that time it is recommended that you discard the paper copy.

In the case of past model year updates, it is recommended that this bulletin be retained with the appropriate model year labor time guide as a complete revision will not be provided.

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N T U W NUMBER VIN CODE

FINESSE SAND AND BUFF A0110 .3 .3 .3 .3 .3 .3 .3 .3 .3 GB GB GB GB GB GB GB GB GB

#### NOTE: Applicable model year: 1990 ADD: A- For Each Additional Panel .1 .1 .1 .1 .1 .1 .1 .1 .1 GA GA GA GA GA GA GA GA GA

BRACKET, FRONT LICENSE PLATE B0140 .2 MOUNTING - REPLACE NOTE: Applicable model years: 1988-90

GLASS, QUARTER STATIONARY - R&R OR REPLACE NOTE: Applicable model years: 1989-90 (2 Door) RIGHT C0510 1.5 LEFT C0511 1.5

TRIM ASSEMBLY, FRONT DOOR - R&R OR REPLACE NOTE: Applicable model year: 1989 RIGHT ONE PIECE C3348 .4 LEFT ONE PIECE C3358 .4 ADD: A- W/REMOTE CONTROL MIRROR .2 B- W/POWER WINDOW .3 C- TO TRANSFER FINISHING MOLDINGS AND/OR PULL HANDLE .2

CARPET, FLOOR - R&R OR REPLACE NOTE: Applicable model year: 1989 ONE PIECE C4208 1.4 ADD: A- W/CONSOLE .6

DEFLECTOR, AIR - REPLACE NOTE: Applicable model years: 1989-90 RIGHT D1440 1.5 LEFT D1441 .3 CENTER D1446 .3

HARNESS, VACUUM HOSE - R&R OR REPLACE NOTE: Applicable model year: 1989 MAIN HARNESS D1705 1.0

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N T U W NUMBER VIN CODE

HOSES, HEATER (WITH AIR CONDITIONING) - REPLACE NOTE: Applicable model year: 1989 V-8 w/ Port Fuel Injection ALL HOSES D2787 1.0

HOSES AND/OR LINES, REFRIGERANT - REPLACE NOTE: Applicable model year: 1989 COMPRESSOR SUCTION AND DISCHARGE D3088 .5 HOSE ASSEMBLY

WHEEL ALIGNMENT - CHECK AND/OR E2020 .6 ADJUST NOTE: Applicable model year: 1988 NOTE: These changes also apply to T1430. ADD: A- To Adjust Rear Suspension Camber (One Side) Exc Auxiliary Rear Spring 1.0 With Auxiliary Rear Spring 1.2 B- To Adjust Rear Suspension Camber (Both Sides) Exc Auxiliary Rear Spring 1.7 With Auxiliary Rear Spring 2.0 C- To Adjust Rear Suspension Toe (Both Sides) .2

PULLEY, POWER STEERING PUMP E8360 .7 .7 - REPLACE NOTE: Applicable model years: 1988-89 w/ OHC-4

CONTROL ASSEMBLY, PARKING BRAKE H2840 .9 - REPLACE NOTE: Applicable model years: 1987-88

SPRING, CAP AND/OR SEAL, VALVE - REPLACE INC: R&R intake manifold. NOTE: Applicable model years: 1987-90 W/ V-6 ONE CYL RIGHT BANK J0540 3.2 BOTH BANKS J0547 3.4

COIL, DISTRIBUTOR - REPLACE J4340 .7 NOTE: Applicable model years: 1987-88 w/ V-6

SENSOR, EGR - REPLACE J6377 1.9 NOTE: Applicable model year: 1985 V-8 w/ Port Injection

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N T U W NUMBER VIN CODE

NEEDLE AND/OR ASSEMBLY, SHIFT RANGE INDICATOR REPLACE K5100 NOTE: Applicable model year: 1988 COLUMN MOUNTED .5 .5 FLOOR MOUNTED .5

SWITCH - REPLACE ENGINE OIL PRESSURE N2220 .4

#### NOTE: Applicable model years: 1988-90 w/ L-4

KEY WARNING N2330 .8 NOTE: Applicable model years: 1988-90

ACTUATOR ASSEMBLY - REPLACE NOTE: Applicable model years: 1988-90

REAR COMPARTMENT LID RELEASE N3270 .3

MOTOR, WIPER - R&R NOTE: Applicable model years: 1988-90 WINDSHIELD N3510 .4

MOTOR, WIPER - REPLACE NOTE: Applicable model years: 1988-90 WINDSHIELD N3520 .4

SPEAKER, RADIO - REPLACE NOTE: Applicable model years: 1988-90 FRONT RIGHT R0940 .6 LEFT R0941 .6

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.