For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment lid release switch, if equipped. Refer to Rear Compartment Lid Switch Replacement .
2. Remove the I/P knee bolster bolts (3).
3. Remove the I/P driver knee bolster (2).

### Installation Procedure

1. Install the I/P driver knee bolster (2).
2. Install the I/P knee bolster bolts (3).

Tighten
Tighten the I/P knee bolster bolts (3) to 1.9 N·m (17 lb in).

3. Install the rear compartment lid release switch, if equipped. Refer to Rear Compartment Lid Switch Replacement .