For 1990-2009 cars

#### Tools Required

J 43276 Clutch Pilot Bearing Remover

Notice: When using the J 43276 Clutch Pilot Bearing Remover, always secure the J 43276-1 Clutch Pilot Bearing Remover tool body using a wrench. Do not allow the J 43276-1 tool body to rotate. Failing to do so causes damage to the J 43276-1 tool body.

1. Remove the clutch pilot bearing using the J 43276 .

1.1. | Install the J 43276-1 into the clutch pilot bearing.

1.2. | Using a wrench, secure the J 43276-1.

1.3. | Insert the J 43276-2 into the J 43276-1.

1.4. | Rotate the J 43276-2 clockwise into the J 43276-1 until the clutch pilot bearing is completely removed from the crankshaft.

1.5. | Rotate the J 43276-2 counterclockwise to remove the J 43276-2 from the J 43276-1.

1.6. | Remove the J 43276-1 from the tool body.

2. Discard the pilot bearing.