For 1990-2009 cars

1. Use feeler gauges to check the 3rd and 4th clutch plate travel.
2. Check the travel between the selective backing plate (655) and the first fiber plate assembly (654A).

The 3rd and 4th clutch plate travel should be 0.90-2.10 mm (0.035-0.083 in).

3. Select the proper 3rd and 4th clutch selective backing plate to obtain the correct travel. Refer to Third and Fourth Clutch Backing Plate Selection .