For 1990-2009 cars

# DOOR GLASS SCRATCHING

#### SUBJECT: DOOR GLASS SCRATCHING (REPLACE DOOR GLASS AND OUTER BELT SEAL STRIP)

#### MODELS: 1993-95 CHEVROLET CAMARO 1993-95 PONTIAC FIREBIRD

#### CONDITION:

SOME OWNERS MAY COMMENT ABOUT SCRATCHES ON THE DOOR GLASS (DEPENDING ON A NUMBER OF FACTORS INCLUDING CLEANLINESS, AMOUNT OF GLASS CYCLES, ETC.).

#### CORRECTION:

WHEN REPLACING THE DOOR GLASS, UNDER WARRANTY, FOR THIS CONDITION, ALSO REPLACE THE OUTER BELT SEAL STRIP.

#### PARTS INFORMATION:

PART NUMBER DESCRIPTION =========== ===========

10255500 DOOR GLASS (RH) 10255501 DOOR GLASS (LH) 10284222 OUTER BELT SEALING STRIP (RH) 10284223 OUTER BELT SEALING STRIP (LH)

PARTS ARE EXPECTED TO BE AVAILABLE ON FEBRUARY 19, 1996.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: C0114 (RH) C0115 (LH) USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.