For 1990-2009 cars

### Removal Procedure

1. Open the I/P compartment door.
2. Remove the contents of the I/P compartment.
3. Remove the I/P compartment hinge screws.
4. Remove the I/P compartment door from the I/P.

### Installation Procedure

1. Install the I/P compartment door to the I/P.
2. Install the I/P compartment hinge screws.

Tighten
Tighten the I/P compartment hinge screws to 2.8 N·m (25 lb in).

3. Install the contents of the I/P compartment.
4. Close the I/P compartment door.