For 1990-2009 cars
ABS Components
ABS/TCS Schematics
Handling ESD Sensitive Parts Notice
Power Distribution Schematics

### Circuit Description

The Outlet valve solenoid circuits are supplied with battery power when the ignition is in the RUN position. The EBCM/EBTCM controls the valve functions by grounding the circuit when necessary.

### Conditions for Setting the DTC

The EBCM/EBTCM senses a discrepancy such as an open, short to ground, or short to voltage in the circuit.

### Action Taken When the DTC Sets

• | A malfunction DTC is stored.

• | ABS/TCS disabled

• | ABS/TCS Indicators are turned on.

• | The Red BRAKE Warning Indicator turns on.

### Conditions for Clearing the DTC

• | Condition for DTC is no longer present and scan tool clear DTC function is used.

• | 100 ignition cycles pass with no DTC detected.

### Test Description

The numbers below refer to step numbers on the Diagnostic Table.

1. This step determines if the DTC is current.

#### DTC C0075 RF ABS Solenoid #2 Circuit Malfunction

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Diagnostic System Check performed? | -- | Go to Step 2 | Go to Diagnostic System Check
2 |

1. Turn the ignition switch to the OFF position.
2. Install a scan tool.
3. Turn the ignition switch to the RUN position, engine off.
4. Using the scan tool run the Automated test.

Does DTC C0075 reset as a current DTC?

--

Go to Step 3

Go to Diagnostic System Check

3 | Replace the EBCM/EBTCM. Refer to Electronic Brake Control Module Replacement . Is the repair complete? | -- | Go to Diagnostic System Check | --