For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the retainers (2). attaching the hood insulator (1) to the hood.
3. Remove the hood insulator (1) from the vehicle.

### Installation Procedure

1. Install the hood insulator (1) to the vehicle.
2. Install the retainers (2).

Install the retainers at the front of the hood insulator (1) and work rearward. Refer to Body Front End Description .

3. Close the hood.