For 1990-2009 cars

## Radiator Air Baffle Assemblies and Deflectors Lower

### Removal Procedure

1. Remove the air lower deflector screws (3).
2. Remove the radiator air lower baffle retainers (4).
3. Remove the radiator air lower baffle (1).
4. Inspect for any component damage.

### Installation Procedure

1. Install the radiator air lower baffle (1).
2. Install the radiator air lower baffle retainers (4).
3. Install the radiator air lower deflector screws (3).

Tighten
Tighten the air lower deflector screws to 10 N·m (89 lb in).

## Radiator Air Baffle Assemblies and Deflectors Upper

### Removal Procedure

1. Remove the radiator air upper baffle from the retainers (3).
2. Remove the radiator air upper baffle (1) from the radiator (2).

### Installation Procedure

1. Install the radiator air upper baffle (1) to the radiator (2).
2. Install the radiator air upper baffle to the retainers (3).