For 1990-2009 cars

### Removal Procedure

1. Remove the I/P carrier. Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges and Console.
2. Place the I/P carrier face down on a clean work surface.
3. Unsnap the side window defogger outlet duct from the air distributor.

### Installation Procedure

1. Snap the side window defogger outlet duct to the air distributor.
2. Install the I/P carrier. Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges and Console.