For 1990-2009 cars

Notice: Routine inspection of the belt may reveal cracks in the belt ribs. These cracks will not impair the belt performance. The belt should be replaced if the belt slip occurs if a section of the belt ribs are missing. A single serpentine drive belt is used to drive all engine accessories. All belt driven accessories are rigidly mounted with the belt tension maintained by a spring loaded tensioner. The indicator on the movable portion of the tensioner must be within the limits of the marks of the stationary portion of the tensioner. Any reading outside of these limits indicates either a defective belt or tensioner.

Inspect the belt length scale on the drive belt tensioner for proper installed length. If the belt length scale does not indicate proper installed length, install a new drive belt.