For 1990-2009 cars

Step | Action | Value | Yes | No
--- | --- | --- | --- | ---
DEFINITION: The transmission cannot be shifted out of gear.
1 | Remove the transmission. Refer to Transmission Removal or to Transmission Removal . Are the gearshift components properly assembled? | -- | Go to Step 2 | Go to Step 3
2 | Are the gearshift components worn, bent, or broken? | -- | Go to Step 4 | Go to Step 5
3 | Disassemble the gearshift components. Properly assemble the gearshift componentsRefer to Transmission Disassemble or to Transmission Disassemble . Will the transmission shift gears? | -- | System OK | Go to Step 5
4 | Replace the worn or damaged parts. Refer to Transmission Disassemble or to Transmission Disassemble . Will the transmission shift gears? | -- | System OK | Go to Step 5
5 | Disassemble the transmission geartrain. Refer to Transmission Disassemble . or to Transmission Disassemble . Look for worn, broken, or, damaged components. Replace all worn, broken, or damaged components. | -- | -- | --