For 1990-2009 cars

# SRTA PROGRAM INTRODUCTION PROCESSING PROCEDURE OUTLINED

TRANSMISSION APPLICATIONS: 200-4R

#### SUBJECT: SERVICE REPLACEMENT TRANSMISSION ASSEMBLY (SRTA) PROGRAM INTRODUCTION

#### TRANSMISSION MODELS:

VEHICLE APPLICATIONS: ALL 1982-90 CARS W/200-4R

#### BULLETIN COVERS:

The THM 200-4R Service Replacement Transmission Assembly (SRTA) Program beginning March 15, 1990. SRTA models can be ordered for all 1982-1990 models from your local General Motors Service Parts Operation (CANSPO)

#### SRTA ADVANTAGES:

- A SRTA is the product of a highly successful, customer satisfaction driven program that parallels the existing HYDRA-MATIC 3T40, HYDRA-MATIC 4T60 and HYDRA-MATIC 4L60 programs. It provides the technician with a service alternative when addressing diagnostic and overhaul concerns.

- All SRTA units are designed and remanufactured to current engineering specifications and are often less costly than a major overhaul.

- IN THE INTEREST OF CUSTOMER SATISFACTION, SRTA MODELS SHOULD ONLY BE CONSIDERED WHEN THE PROJECTED COST OF REPAIR EXCEEDS THE COST OF A SRTA REPLACEMENT.

#### GENERAL GUIDELINES:

o Replacement or Overhaul:

Parts needed to perform unit replacement or internal overhaul on a THM 200-4R transmission are available through your local Parts Distribution Centre (PDC).

- Transmission conditions considered for SRTA usage: o All repairs in which the projected cost to repair exceeds the cost of SRTA replacement. o Indications that major internal repair is required.

- Dealer THM 200-4R transmission repairs include: o All on-vehicle serviceable items. o All internal repairs which are projected to cost less than a SRTA replacement.

#### COOLER FLUSHING:

#### IMPORTANT: Cooler flushing MUST be performed whenever a transmission/ transaxle is removed for service. It is essential to flush the cooler after SRTA installation, major overhaul, in any case of pump or torque converter replacement, or when fluid contamination is suspected. Use Kent-Moore tool J-35944 to flush the cooler.

#### SRTA PROCESSING PROCEDURE:

Each SRTA unit will be shipped in a container which must be used for core return of the original THM 200-4R assembly. A SRTA Information Packet is included with each SRTA unit. The contents of this envelope are to be removed and used as described with each illustration on the following pages.

** FIGURE 1 **

#### SRTA PROCESSING PROCEDURES - INFORMATION PACKET:

The contents of this envelope include Limited Warranty Information, Dealer Product Feedback Form, Core Exchange Return Procedure, and a pre-addressed return mailing envelope. A dealer representative is to explain to the customer all warranty information about the SRTA contained in this envelope.

** FIGURE 2 **

#### SRTA PROCESSING PROCEDURES - CORE EXCHANGE RETURN:

The core return procedure provides detailed instructions for the GM dealer on handling the SRTA and original THM 200-4R units. This sheet can be discarded after use.

** FIGURE 3 **

#### SRTA PROCESSING PROCEDURES - FAILURE ANALYSIS INFORMATION:

This Product Feedback Form is to be completed by the service manager and/or technician. Fill out this form as completely as possible to provide information which can be used for analysis. This valuable input can result in future product refinement through corrective action. Insert the white copy of the completed form and a copy of the repair order into the SRTA Information Packet envelope, reseal the envelope and wire tag it to the bell housing of the unit being returned for core exchange. Return the yellow copy of the completed Product Feedback form, using the postage paid envelope, to Hydra-matic Division.

** FIGURE 4

#### THM 200-4R TRANSMISSION IDENTIFICATION INFORMATION:

Transmission identification information and the SRTA model replacement chart will assist in selecting the correct SRTA unit to order from your local Parts Distribution Centre.

** FIGURE 5 **

#### THM 200-4R SRTA MODEL REPLACEMENT CHART:

#### ORIGINAL TRANSMISSION MODEL YEAR AND MODEL

SRTA SRTA PART MODEL 1982 1983 1984 1985 1986 1987 1988 1989 1990

8669944 4BQ 3BR 4BQ 8669945 4BT 4BT 8639972 4BY 3BY 4BY 8669947 4CR 9CR 4CR 8669948 40J 40J 8669949 40M 90M 30M 40M 8669939 5HE 9HE,9HG 4HE 5HE 8669941 50G 90G 30G 40G 50G 8669942 50J 50J 8669943 50M 50M 8669940 5HG 4HG 5HG 8669937 5BQ 5BQ 8669938 5CH 4CH 5CH

SRTA SRTA PART # MODEL 1982 1983 1984 1985 1986 1987 1988 1989 1990

8669925 6AA 9AA 3AA 4AA 5AA 6AA 8669926 6AB 5AC 6AB 8669927 6AP 9AP 3AP 4AP 5AP 6AP 8669928 6CA 6CA 8669929 6CH 5CY 6CH 8669930 6CR 5CR 6CR 8669931 6CZ 4CQ 5CQ 6CZ 8669932 6HC 6HC 8669933 6KB 6KB 8669934 6KC 6KC 8669935 6KJ 6KJ 8669936 6KZ 30Z 40Z 50Z 6KZ 8669923 7HT 7HT 8669922 7HF 7HF 8669924 7KC 7KC 8669916 7CC 7CC 8639965 7CZ 7CZ 8669921 7HD 7HD 8639967 7KZ 7KZ 8669920 7CY 7CY 8669918 7CR 7CR 8639966 7BR 7CT 8CT 8669909 8CH 7CH 8CH 8669915 8CZ 8CZ 8669912 8CR 8CR 8669908 8CC 8CC 8669914 8CY 8CY 8669902 9TA 9TA 8669905 OKD OKD 8669903 OCT 9CT OCT 8669904 OCU 9CU OCU 8669907 OKT 7KT 8KT 9KT OKT 8669906 OKJ 7KJ 8KJ 9KJ OKJ

#### PARTS INFORMATION:

- Part numbers are accurate at the time of printing and subject to change.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.