For 1990-2009 cars

Important: Do not reuse the engine coolant air bleed pipe gaskets. Upon installation of the pipe, install NEW gaskets.

1. Remove the engine coolant air bleed hose, clamps and sealing gaskets from the pipe.
2. Clean the pipe and hose in solvent.

Caution: Wear safety glasses in order to avoid eye damage.

3. Dry the pipe with compressed air.
4. Inspect the pipe for damage or restrictions.
5. Inspect the pipe gasket and hose sealing surfaces for damage.
6. Inspect the pipe hose for restrictions, cracking or wear.

The pipe hose may be reused if not damaged.