For 1990-2009 cars

## Converter Hanger Assembly Replacement 3.8L Automatic

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Support the catalytic converter.
3. Remove the catalytic converter hanger bolts.
4. Remove the catalytic converter hanger from the front hanger bracket.
5. Remove the rear axle torque arm nuts.
6. Remove the rear axle torque arm inner bracket bolts.
7. Remove the catalytic converter front hanger bracket from the vehicle.

### Installation Procedure

1. Install the catalytic converter front hanger bracket to the vehicle.
2. Install the rear axle torque arm inner bracket bolts.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the rear axle torque arm nuts.

Tighten
Tighten the rear axle torque arm nuts to 45 N·m (33 lb ft).

4. Install the catalytic converter hanger to the front hanger bracket.
5. Install the catalytic converter hanger bolts.

Tighten
Tighten the catalytic converter hanger bolts to 41 N·m (30 lb ft).

6. Remove the support from the catalytic converter.
7. Lower the vehicle.

## Converter Hanger Assembly Replacement 5.7L Auto/Man

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Support the catalytic converter.
3. Remove the catalytic converter hanger bolts.
4. Remove the hanger from the bracket.
5. Remove the rear axle torque arm bracket nuts.
6. Remove the catalytic converter hanger bracket.

### Installation Procedure

1. Install the catalytic converter hanger to the bracket.
2. Install the catalytic converter bracket to the rear axle torque arm inner bracket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the rear axle torque arm bracket nuts.

Tighten
Tighten the rear axle torque arm bracket nut to 41 N·m (30 lb ft).

4. Install the catalytic converter hanger bolts.

Tighten
Tighten the converter hanger bolts to 41 N·m (30 lb ft).

5. Remove the support from the catalytic converter.
6. Lower the vehicle.

## Converter Hanger Assembly Replacement 3.8L Man

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Support the catalytic converter.
3. Remove the catalytic converter hanger bolts.
4. Remove the hanger from the bracket.
5. Remove the rear axle torque arm bracket nuts.
6. Remove the catalytic converter front hanger bracket.

### Installation Procedure

1. Install the catalytic converter front hanger bracket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the rear axle torque arm bracket nuts.

Tighten
Tighten the rear axle torque arm bracket nut to 45 N·m (33 lb ft)

3. Install the hanger to the bracket.
4. Install the catalytic converter hanger bolts.

Tighten
Tighten the converter hanger bolts to 41 N·m (30 lb ft)

5. Remove the support from the catalytic converter.
6. Lower the vehicle.