For 1990-2009 cars

## Drive Belt Idler Pulley Replacement Accessory

### Removal Procedure

1. Remove the accessory drive belt. Refer to Drive Belt Replacement .
2. Remove the drive belt idler pulley bolt.
3. Remove the drive belt idler pulley.

### Installation Procedure

1. Install the drive belt idler pulley.

Important: Be sure the idler pulley is fully seated against the shoulder on the generator bracket before tightening the bolt.

2. Install the drive belt idler pulley bolt.

Tighten
Tighten the drive belt idler pulley bolt to 50 N·m (37 lb ft).

3. Install the accessory drive belt. Refer to Drive Belt Replacement .

## Drive Belt Idler Pulley Replacement A/C

### Removal Procedure

1. Remove the air conditioning (A/C) drive belt. Refer to Drive Belt Replacement .
2. Remove the A/C drive belt idler pulley bolt (2).
3. Remove the A/C drive belt idler pulley (1).

### Installation Procedure

1. Install the A/C drive belt idler pulley (1).

Important: Be sure the idler pulley is fully seated against the shoulder on the A/C compressor bracket before tightening the bolt.

2. Install the A/C drive belt idler pulley bolt (2).

Tighten
Tighten the A/C drive belt idler pulley bolt to 50 N·m (37 lb ft).

3. Install the A/C drive belt. Refer to Drive Belt Replacement .