For 1990-2009 cars

### Purpose

Varying octane levels in today's gasoline may cause detonation in some engines. Detonation is caused by an uncontrolled explosion (burn) in the combustion chamber. This uncontrolled explosion could produce a flame front opposite that of the normal flame front produced by the spark plug. The rattling sound normally associated with detonation is the result of two or more opposing pressures (flame fronts) colliding within the combustion chamber. Though light detonation is sometimes considered normal, heavy detonation could result in engine damage. To control spark knock, a Knock Sensor (KS) system is used. This system is designed to retard spark timing when spark knock is detected in the engine. The KS system allows the engine to use maximum spark advance for optimal driveability and fuel economy.

### Operation

The PCM contains integrated Knock Sensor (KS) Diagnostic Circuitry. Input signals from the knock sensors are used to detect engine detonation, allowing the PCM to retard Ignition Control (IC) spark timing based on the amplitude and frequency of the KS signal being received. The knock sensors produce an AC signal under all engine operating conditions. The PCM calculates an average voltage of each knock sensor's signal and takes instantaneous signal voltage readings. The PCM uses the instantaneous signal voltage readings to determine the state of the knock sensor circuitry. If the knock sensor system is operating normally, the PCM should monitor instantaneous KS signal voltage readings varying outside a voltage range above and below the calculated average voltage(as shown in the normal knock sensor figure). If the PCM detects a knock sensor signal voltage within the calculated average voltage range, DTC P0327 or P0332 will set (as shown in the abnormal knock sensor figure).

(1) | Upper Fail Region
(2) | Knock Sensor Calculated Average
(3) | Knock Sensor Signal (Normal)
(4) | Lower Fail Region

(1) | Upper Fail Region
(2) | Knock Sensor Calculated Average
(3) | Knock Sensor Signal (Failed)
(4) | Lower Fail Region

### Diagnosis

If the PCM malfunctions in a manner which will not allow proper diagnosis of the knock sensor system, DTC P0325 will set.

DTCs P0327 and P0332 are designed to diagnose the knock sensors, and related wiring. Problems encountered with the KS system should set a DTC. However, if the customer's complaint is detonation/spark knock, use the tables for DTC P0327 or P0332 to diagnose the condition.