For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the license pocket cover screws.
3. Remove the license pocket cover from the vehicle.

### Installation Procedure

1. Install the license pocket cover to the vehicle.
2. Install the license pocket cover screws.

Tighten
Tighten the license pocket cover screws to 2.0 N·m (18 lb in).

3. Lower the vehicle.