For 1990-2009 cars

### Removal Procedure

1. Unsnap the rear compartment lamp from the rear finish panel.
2. Disconnect the electrical connector from the lamp.
3. Push the top of the rear compartment lamp bulb down in order to remove the bulb from the clips.

### Installation Procedure

1. Install the rear compartment lamp bulb to the lamp by performing the following actions:

1.1. | Push the top of the metal strip down.

1.2. | Attach the bulb to the clips.

2. Connect the electrical connector to the lamp.
3. Snap the rear compartment lamp to the rear finish panel.