For 1990-2009 cars

Many features of the universal theft deterrent system, including horn chirps, how the system arms and delay times, may be set to the customer's preference. The alarm system can also be turned off. To customize features, after the system is in programming mode, refer to the appropriate chart below.

### Programming Mode

Programming mode is necessary to customize features of the system. To set body control module (BCM) in programming mode, refer to the following procedure.

### Entering Programming Mode

To enter the programming mode, perform the following:

1. Turn the ignition ON.

This will disarm the theft system, if necessary.

2. Turn the ignition OFF.
3. Remove the RADIO fuse (# 17).
4. Turn the ignition to the ACC position.

The chime will sound to verify the system is in programming mode.

• | When the chime sounds once; exit lighting, delayed illumination, last door closed locking and unlocking prevention can be customized.

• | When the chime sounds twice and the vehicle is equipped with universal theft deterrent; remote lock control verification, arming method, arming verification, driver's door delay and shock sensor enable/disable can be customized.

### Exiting Programming Mode

To exit the programming mode, perform the following:

1. When the programming is done, turn the ignition switch OFF.
2. Install the RADIO fuse (# 17).

### Customization Charts

#### Exit Lighting and Delayed Illumination

Exit lighting illuminates interior lamps when the key is removed from the ignition switch to help in exiting the vehicle. Delayed illumination illuminates interior lamps for 25 seconds after the doors are closed. The 25 seconds is shortened if the ignition is turned on or if the power locks are activated. Both exit lighting and delayed illumination are enabled from the factory, and can be disabled if desired.

1. Enter the programming mode.
2. Turn the courtesy lamp switch ON then OFF (I/P dimmer switch, not parking lamps).

Listen to the number of chimes to determine current setting.

The factory setting is in CAPITAL print.

3. Turn the courtesy lamp switch ON and OFF to increment desired setting below.
4. Continue customizing other features or exit the programming mode.

Number of Chimes | Exit Lighting Feature | Delayed Illumination Feature
--- | --- | ---
1 | Disabled | Disabled
2 | Disabled | Enabled
3 | Enabled | Disabled
4 | ENABLED | ENABLED

#### Last Door Closed Locking and Lockout Prevention

Last door closed locking is available on cars with power locks, this feature provides for delayed locking of the door (three seconds after the last door is closed). This allows the driver to exit the vehicle and press the lock button (either on the key fob or the door panel), but the doors will not lock until both doors are closed. When the locked switch is pressed, the chime will sound three times, indicating a last door closed locking is pending. Pressing the lock switch again will lock the doors immediately. Pressing the unlock switch will cancel a pending last door closed locking. Last door closed locking is disabled from the factory, and can be enabled if desired.

Lockout prevention protects the driver from locking the keys in the vehicle, this feature disables the power lock from locking when the keys are in the ignition and a door is open. If the power lock button is pressed when a door is open, the chime will sound 5 times as a reminder to take the keys before locking the door. Lockout prevention is enabled from the factory, and can be disabled if desired.

1. Enter the programming mode.
2. Press the lock switch on the door.

Listen to the number of chimes to determine current setting.

The factory setting is in CAPITAL print.

3. Press the lock switch on the door to increment desired setting below.
4. Continue customizing other features or exit the programming mode.

Number of Chimes | Last Door Closed Locking | Lockout Prevention
--- | --- | ---
1 | Disabled | Disabled
2 | DISABLED | ENABLED
3 | Enabled | Disabled
4 | Enabled | Enabled

#### Remote Lock Control Verification (Horn Chirp and Parking Lamps Flash)

Available on vehicles equipped with Universal Theft Deterrent (UTD) system, this feature provides horn chirps and/or parking lamp illumination to indicate that the remote transmitter LOCK or UNLOCK command was received.

1. Enter the programming mode.
2. Press the unlock switch on the remote transmitter.

Listen to the number of chimes to determine current setting.

The factory setting is in CAPITAL print.

3. Press the unlock switch on the remote transmitter to increment desired setting below.
4. Continue customizing other features or exit the programming mode.

Number of Chimes | Key Fob Lock 1st Push | Key Fob Lock 2nd Push | Key Fob Unlock
--- | --- | --- | ---
1 | Verification Off | Verification Off | Verification Off
2 | Horns and Lamps | Horns and Lamps | Lamps
3 | Horns and Lamps | Horns and Lamps | Horns and Lamps
4 | Lamps | Lamps | Lamps
5 | LAMPS | HORNS AND LAMPS | LAMPS

#### Theft Deterrent Arming Method

Available on vehicles equipped with Universal Theft Deterrent (UTD) system, this feature provides different methods of arming the UTD system.

1. Enter the programming mode.
2. Press the unlock switch on the door.

Listen to the number of chimes to determine current setting.

The factory setting is in CAPITAL print.

3. Press the unlock switch on the door to increment desired setting below.
4. Continue customizing other features or exit the programming mode.

Number of Chimes | Theft Deterrent Arming Method
--- | ---
1 | Alarm System Off
2 | Remote Transmitter Arms
3 | REMOTE TRANSMITTER OR DOOR LOCK SWITCH ARMS
4 | Passive (Automatic)

#### Theft Deterrent Arming Verification (Horn Chirp and Parking Lamps Flash)

Available on vehicles equipped with Universal Theft Deterrent (UTD) system, this feature provides horn chirps and/or parking lamp illumination to indicate when the UTD system has been armed. It is programmed separately from the remote lock control verification list above.

1. Enter the programming mode.
2. Press the lock switch on the remote transmitter.

Listen to the number of chimes to determine current setting.

The factory setting is in CAPITAL print.

3. Press the lock switch on the remote transmitter to increment desired setting below.
4. Continue customizing other features or exit the programming mode.

Number of Chimes | Arming with Key Fob | Arming With Door Lock Switch | Passive Arming
--- | --- | --- | ---
1 | Off | Off | Off
2 | Horns and Lamps | Horns and Lamps | Horns and Lamps
3 | HORNS AND LAMPS | LAMPS | LAMPS
4 | Lamps | Lamps | Lamps

#### Theft Deterrent Operation (Driver's Door Delay and Shock Sensor Enable)

Available on vehicles equipped with Universal Theft deterrent (UTD) system, this feature provides a driver's door delay that can be set at zero or 8 seconds from the time the driver's door is opened until the alarm sounds. The shock sensor feature, that detects sharp blows to the vehicle, can also be enabled or disabled using this chart. Refer to Content Theft Deterrent (CTD) Description for a description of the two sensitivity levels. Refer to Shock Sensor Replacement for adjustment procedures.

1. Enter the programming mode.
2. Turn the parking lamps ON and OFF.

Listen to the number of chimes to determine current setting.

The factory setting is in CAPITAL print.

3. Turn the parking lamps ON and OFF to increment desired setting below.
4. Continue customizing other features or exit programming mode.

Number of Chimes | Drivers Door Delay | Shock Sensor Enable
--- | --- | ---
1 | Zero | Disabled
2 | 8 seconds | Disabled
3 | Zero | Enabled
4 | 8 SECONDS | ENABLED