For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Control Cable Bracket Bolts | 10 N·m | 89 lb in
Air Conditioning Compressor Bolts | 50 N·m | 37 lb ft
Air Conditioning Compressor Bracket Bolts | 50 N·m | 37 lb ft
Air Conditioning Idler Pulley Bolt | 50 N·m | 37 lb ft
Air Conditioning Tensioner Bolt | 25 N·m | 18 lb ft
Air Injection Reaction (AIR) Pipe-to-Exhaust Manifold Bolts | 20 N·m | 15 lb ft
Camshaft Retainer Bolts | 25 N·m | 18 lb ft
Camshaft Sensor Bolt | 25 N·m | 18 lb ft
Camshaft Sprocket Bolts | 35 N·m | 26 lb ft
Catalytic Converter Nut | 25 N·m | 18 lb ft
Connecting Rod Bolts - First Design - First Pass | 20 N·m | 15 lb ft
Connecting Rod Bolts - First Design - Final Pass | 85 degrees
Connecting Rod Bolts - Second Design - First Pass | 20 N·m | 15 lb ft
Connecting Rod Bolts - Second Design - Final Pass | 85 degrees
Coolant Temperature Gauge Sensor | 20 N·m | 15 lb ft
Crankshaft Balancer Bolt (Installation Pass-to Ensure the Balancer is Completely Installed) | 330 N·m | 240 lb ft
Crankshaft Balancer Bolt (First Pass-Install a NEW Bolt After the Installation Pass and Tighten as Described in the First and Final Passes) | 50 N·m | 37 lb ft
Crankshaft Balancer Bolt (Final Pass) | 140 degrees
Crankshaft Bearing Cap Bolts (Inner Bolts-First Pass in Sequence) | 20 N·m | 15 lb ft
Crankshaft Bearing Cap Bolts (Inner Bolts-Final Pass in Sequence) | 80 degrees
Crankshaft Bearing Cap Side Bolts | 25 N·m | 18 lb ft
Crankshaft Bearing Cap Studs (Outer Studs-First Pass in Sequence) | 20 N·m | 15 lb ft
Crankshaft Bearing Cap Studs (Outer Studs-Final Pass in Sequence) | 53 degrees
Crankshaft Oil Deflector Nuts | 25 N·m | 18 lb ft
Crankshaft Position Sensor Bolt | 25 N·m | 18 lb ft
Cylinder Head Bolts (First Pass all M11 Bolts in Sequence) | 30 N·m | 22 lb ft
Cylinder Head Bolts (Second Pass all M11 Bolts in Sequence) | 90 degrees
Cylinder Head Bolts (Final Pass all M11 Bolts in Sequence-Excluding the Medium Length Bolts at the Front and Rear of Each Cylinder Head) | 90 degrees
Cylinder Head Bolts (Final Pass M11 Medium Length Bolts at the Front and Rear of Each Cylinder Head in Sequence) | 50 degrees
Cylinder Head Bolts (M8 Inner Bolts in Sequence) | 30 N·m | 22 lb ft
Cylinder Head Coolant Plug | 20 N·m | 15 lb ft
Cylinder Head Core Hole Plug | 20 N·m | 15 lb ft
Drive Belt Idler Pulley Bolt | 50 N·m | 37 lb ft
Drive Belt Tensioner Bolts | 50 N·m | 37 lb ft
Engine Block Coolant Drain Plugs | 60 N·m | 44 lb ft
Engine Block Heater | 40 N·m | 30 lb ft
Engine Block Oil Gallery Plugs | 60 N·m | 44 lb ft
Engine Crossmember Bolts (Large) | 145 N·m | 107 lb ft
Engine Crossmember Bolts (Small) | 125 N·m | 92 lb ft
Engine Flywheel Bolts (First Pass) | 20 N·m | 15 lb ft
Engine Flywheel Bolts (Second Pass) | 50 N·m | 37 lb ft
Engine Flywheel Bolts (Final Pass) | 100 N·m | 74 lb ft
Engine Flywheel-to-Torque Converter Bolts | 60 N·m | 44 N·m
Engine Front Cover Bolts | 25 N·m | 18 lb ft
Engine Mount Heat Shield Nuts | 10 N·m | 89 lb in
Engine Mount Stud-to Engine Block | 50 N·m | 37 lb ft
Engine Mount Through Bolts | 95 N·m | 70 lb ft
Engine Mount Through Bolt Nuts | 80 N·m | 59 lb ft
Engine Mount-to-Engine Block Bolts | 50 N·m | 37 lb ft
Engine Rear Cover Bolts | 30 N·m | 22 lb ft
Engine Service Lift Bracket M10 Bolts | 50 N·m | 37 lb ft
Engine Service Lift Bracket M8 Bolt | 25 N·m | 18 lb ft
Engine Valley Cover Bolts | 25 N·m | 18 lb ft
Engine Wire Harness Clip Bolt | 50 N·m | 37 lb ft
Engine Wire Harness Ground Strap Bolt | 50 N·m | 37 lb ft
Exhaust Gas Recirculation (EGR) Valve Bolts (First Pass) | 10 N·m | 89 lb in
EGR Valve Bolts (Final Pass) | 30 N·m | 20 lb ft
EGR Valve Pipe-to-Cylinder Head Bolts | 50 N·m | 37 lb ft
EGR Valve Pipe-to-Exhaust Manifold Bolts | 30 N·m | 20 lb ft
EGR Valve Pipe-to-Intake Manifold Bolt | 12 N·m | 106 lb in
Exhaust Manifold Bolts (First Pass) | 15 N·m | 11 lb ft
Exhaust Manifold Bolts (Final Pass) | 20 N·m | 15 lb ft
Exhaust Manifold Pipe Nuts | 35 N·m | 26 lb ft
Front Shock-to-Engine Crossmember Bolts | 65 N·m | 48 lb ft
Fuel Injection Fuel Rail Bolts | 10 N·m | 89 lb in
Generator Bracket Bolts | 50 N·m | 37 lb ft
Generator Rear Bracket-to-Engine Block Bolt | 25 N·m | 18 lb ft
Generator Rear Bracket-to-Generator Bolt | 25 N·m | 18 lb ft
Ground Strap Bolt (at Rear of Cylinder Head) | 50 N·m | 37 lb ft
Ignition Coil-to-Bracket Bolts | 12 N·m | 106 lb in
Ignition Coil Bracket-to-Valve Rocker Arm Cover Bolts | 12 N·m | 106 lb in
Intake Manifold Bolts (First Pass in Sequence) | 5 N·m | 44 lb in
Intake Manifold Bolts (Final Pass in Sequence) | 10 N·m | 89 lb in
Knock Sensors | 20 N·m | 15 lb ft
Oil Filter | 30 N·m | 22 lb ft
Oil Filter Fitting | 55 N·m | 40 lb ft
Oil Level Indicator Tube Bolt | 25 N·m | 18 lb ft
Oil Level Sensor | 13 N·m | 115 lb in
Oil Pan Baffle Bolts | 12 N·m | 106 lb in
Oil Pan Closeout Cover Bolt (Left Side) | 12 N·m | 106 lb in
Oil Pan Closeout Cover Bolt (Right Side) | 12 N·m | 106 lb in
Oil Pan Drain Plug | 25 N·m | 18 lb ft
Oil Pan M8 Bolts (Oil Pan-to-Engine Block and Oil Pan-to-Front Cover) | 25 N·m | 18 lb ft
Oil Pan M6 Bolts (Oil Pan-to-Rear Cover) | 12 N·m | 106 lb in
Oil Pressure Sensor | 20 N·m | 15 lb ft
Oil Pump-to-Engine Block Bolts | 25 N·m | 18 lb ft
Oil Pump Cover Bolts | 12 N·m | 106 lb in
Oil Pump Relief Valve Plug | 12 N·m | 106 lb in
Oil Pump Screen Nuts | 25 N·m | 18 lb ft
Oil Pump Screen-to-Oil Pump Bolt | 12 N·m | 106 lb in
Oil Transfer Cover Bolts | 12 N·m | 106 lb in
Oxygen Sensor | 42 N·m | 31 lb ft
Positive Crankcase Ventilation (PCV) System Strap Nut (at Right Front Vapor Vent Pipe Stud) | 12 N·m | 106 lb in
Power Steering Pump Bolts | 25 N·m | 18 lb ft
Power Steering Pump Bracket Bolts | 25 N·m | 18 lb ft
Spark Plugs (Cylinder Heads-New) | 20 N·m | 15 lb ft
Spark Plugs (all Subsequent Installations) | 15 N·m | 11 lb ft
Throttle Body Bolts | 12 N·m | 106 lb in
Transmission Bellhousing Bolt | 50 N·m | 37 lb ft
Valve Lifter Guide Bolts | 12 N·m | 106 lb in
Valve Rocker Arm Bolts | 30 N·m | 22 lb ft
Valve Rocker Arm Cover Bolts | 12 N·m | 106 lb in
Vapor Vent Pipe Bolts and Studs | 12 N·m | 106 lb in
Water Inlet Housing Bolts | 15 N·m | 11 lb ft
Water Pump Bolts (First Pass) | 15 N·m | 11 lb ft
Water Pump Bolts (Final Pass) | 30 N·m | 22 lb ft
Water Pump Cover Bolts | 15 N·m | 11 lb ft