For 1990-2009 cars

# INFORMATION ON REVISED ALIGNMENT SPECIFICATIONS

#### SUBJECT: INFORMATION ON REVISED ALIGNMENT SPECIFICATIONS

#### MODELS: 1995-96 CHEVROLET CAMARO 1995-96 PONTIAC FIREBIRD

WHENEVER THE ALIGNMENT IS TO BE CHECKED OR RESET FOR ANY REASON, THE FOLLOWING SPECIFICATIONS SHOULD BE USED.

IF THE VEHICLE IS EQUIPPED WITH GOODYEAR EAGLE RSA TIRES, THE FOLLOWING ALIGNMENT SPECIFICATIONS SHOULD BE FOLLOWED:

LEFT RIGHT ==== =====

CASTER 4.00 DEG +/- .5 DEG 4.40 DEG +/- .5 DEG

CAMBER +0.20 DEG +/- .5 DEG -0.20 DEG +/- .5 DEG

SUM TOE 0 DEG +/- .2 DEG

IF THE VEHICLE IS EQUIPPED WITH ANY OTHER TIRES, THE FOLLOWING ALIGNMENT SPECIFICATIONS SHOULD BE FOLLOWED:

CASTER 4.8 DEG +/- .5 DEG

CAMBER .40 DEG +/- .5 DEG

SUM TOE 0 DEG +/- .2 DEG

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: E2020 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.