For 1990-2009 cars

## Radiator Outlet Hose Replacement V6

### Removal Procedure

1. Drain the engine coolant. Refer to Cooling System Draining and Filling .
2. Disconnect the (IAT) intake air temperature sensor electrical connector.
3. Remove the air intake duct.
4. Remove the outlet hose from the water pump.
5. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
6. Remove the outlet hose from the radiator.
7. Remove the hose support from the fan shroud.

### Installation Procedure

1. Install the outlet hose support to the fan shroud.
2. Install the outlet hose to the radiator.
3. Lower the vehicle.
4. Install the outlet hose to the water pump.
5. Install the air intake duct.
6. Connect the IAT sensor electrical connector.
7. Refill the engine coolant. Refer to Cooling System Draining and Filling .

## Radiator Outlet Hose Replacement V8

### Removal Procedure

1. Drain the engine coolant. Refer to Cooling System Draining and Filling .
2. Disconnect the (IAT) intake air temperature sensor and the (MAF) mass airflow sensor electrical connectors.
3. Remove the air intake duct.
4. Remove the outlet hose from the water outlet.
5. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
6. Remove the outlet hose from the radiator.

### Installation Procedure

1. Install the outlet hose to the radiator.
2. Lower the vehicle.
3. Install the outlet hose to the water outlet.
4. Install the air intake duct.
5. Connect the IAT sensor and the MAF sensor electrical connectors.
6. Refill the engine coolant. Refer to Cooling System Draining and Filling .