For 1990-2009 cars

### Removal Procedure

The Clutch Anticipate Switch is located on the Brake/Clutch Pedal Bracket.

1. Remove the left side hush panel.
2. Disconnect the electrical connectors.
3. Grasp and pull the Clutch Anticipate Switch straight out of the retainer.

### Installation Procedure

1. Position the Clutch Anticipate Switch into the Brake/Clutch Pedal Bracket.

• | Hold the clutch pedal depressed while installing the switch.

• | The switch should bottom in the retainer. Note that audible clicks can be heard as the switch is pressed into the retainer.

2. Slowly pull the clutch pedal rearward against the pedal stop.
3. Release the clutch pedal and pull back on it again to ensure proper switch adjustment.
4. Connect the electrical connector.
5. Install the left side hush panel.