For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment lid release switch, if equipped. Refer to Rear Compartment Lid Switch Replacement in Body Rear End.
2. Remove the I/P knee bolster bolts (3).
3. Remove the I/P knee bolster (2).
4. Remove the I/P knee bolster bracket nuts (4).
5. Remove the I/P knee bolster bracket (5).

### Installation Procedure

1. Install the I/P knee bolster bracket (5).
2. Install the I/P knee bolster bracket nuts (4).

Tighten
Tighten the I/P knee bolster bracket nuts (4) to 10 N·m (89 lb in).

3. Install the I/P knee bolster (2).
4. Install the I/P knee bolster bolts (3).

Tighten
Tighten the I/P knee bolster bolts (3) to 1.9 N·m (17 lb in).

5. Install the rear compartment lid release switch, if equipped. Refer to Rear Compartment Lid Switch Replacement in Body Rear End.