For 1990-2009 cars

# INFO. ON SHIFT CONTROL CABLE INSTALLATION PROCEDURES

#### SUBJECT: INFORMATION ON SHIFT CONTROL CABLE INSTALLATION PROCEDURES

#### MODELS AFFECTED: 1984-93 FIREBIRD MODELS (4L60)

This service bulletin is to emphasize the proper care required to remove or install the automatic transmission shift control cable per Section 7A of the applicable service manual.

When removing or installing the shift control cable (2) from the shift control bracket (3), do NOT bend or twist the molded end. The molded end must be inserted or pulled out straight from the shift control bracket (3).

Failure to follow the above precautions may damage the shift control cable (2).

After the installation of the shift control cable (2), inspect for any damage to the cable.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.