For 1990-2009 cars

#### Tools Required

• | J 25025-5 Guide Pins

• | J 36850 Assembly Lubricant

1. Inspect the valve body spacer plate and the solenoid screens (49, 50) for damage or debris.

Replace the solenoid screens (49, 50) if necessary.

2. Install the #1 checkball into the case.
3. Install the J 25025-5 into the case.
4. Place the spacer plate to case gasket (47) (identified by a "C") and the spacer plate to valve body gasket (52) (identified by a "V") on the spacer plate (48). Retain gaskets on the spacer plate with J 36850 or equivalent.
5. Place the spacer and the spacer plate gaskets on the case.
6. Install the spacer plate support plate (53).
7. Install the spacer plate support bolts (77).
8. Install the 1-2 accumulator housing assembly (57).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

9. Install the 1-2 accumulator housing bolts (58, 59).

Tighten
Tighten the bolts to 11 N·m (8 lb ft).