For 1990-2009 cars

## Ignition Coil and Ignition Coil Module Assemble L36

### Disassembly Procedure

1. Install the ignition control module to the ignition control module bracket.
2. Install the ignition coil seals and the ignition coils to the ignition control module.
3. Install the ignition coil bolts.

Tighten
Tighten the bolts to 45 N·m 40 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

## Ignition Coil and Ignition Coil Module Assemble LT1

### Assembly Procedure

Notice: A package of silicone grease is included with a new ICM. This grease is necessary for ignition coil and ICM cooling.

1. Apply silicone grease to the ignition coil mating surfaces.
2. Install the ICM.
3. Install the ICM screws.

Tighten
Tighten the screws to 1.7 N·m (15 lb in).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the ignition coil.
5. Install the new ignition coil screws.

Tighten
Tighten the screws to 2.8 N·m (25 lb in.).