For 1990-2009 cars

Important: Note the position and direction of the engine flywheel before removal. The flywheel does not use a locating pin for alignment and will not initially seat against the crankshaft flange, but will be pulled onto the crankshaft by the engine flywheel bolts. This procedure requires a three stage tightening process.

1. Remove the engine flywheel bolts.
2. Remove the automatic transmission engine flywheel, if applicable.
3. Remove the manual transmission engine flywheel, if applicable.