For 1990-2009 cars

### Removal Procedure

1. Reposition the brake booster vacuum hose clamps.
2. Remove the hose clamp from the engine side of the vacuum hose, if equipped.
3. Remove the power brake booster vacuum hose from the engine fitting and the vacuum check valve.
4. Remove the vacuum hose.

### Installation Procedure

1. Install the vacuum hose .
2. Connect the power brake booster vacuum hose to the engine fitting and the vacuum check valve.
3. Install the hose clamp to the engine side of the vacuum hose. if equipped.
4. Reposition the brake booster vacuum hose clamps.