For 1990-2009 cars

#### Tools Required

• | J 8092 Driver Handle

• | J 23062-14 Bearing and Bushing Remover/Installer

• | J 21426 Rear Extension Housing Seal Installer

1. Install a new bushing in the extension housing using the J 23062-14 and the J 8092 .
2. Install a new extension housing oil seal using the J 21426 .
3. Lubricate the inside diameter of the extension housing oil seal with DEXRON III® or equivalent.