For 1990-2009 cars

## Door Lamp Replacement Chevrolet

### Removal Procedure

1. Remove the door switch panel from the door.
2. Disconnect the switches electrical connectors.
3. Remove the inside handle bezel screws.
4. Remove the inside handle bezel.
5. Disconnect the harness socket from the bezel.
6. Remove the bulb from the socket.

### Installation Procedure

1. Install the bulb to the socket.
2. Connect the harness socket to the bezel.
3. Install the inside handle bezel.
4. Install the inside handle bezel screws.

Tighten
Tighten the inside handle bezel screws to 1.4 N·m (12 lb in).

5. Connect the switches electrical connectors.
6. install the door switch panel to the door.

## Door Lamp Replacement Pontiac

### Removal Procedure

1. Remove the door switch panel from the door.
2. Disconnect the switches electrical connectors.
3. Remove the inside handle bezel screw.
4. Remove the inside handle bezel.
5. Disconnect the socket from the inside handle bezel.
6. Remove the bulb from the socket.

### Installation Procedure

1. Install the bulb to the socket.
2. Install the socket to the inside handle bezel.
3. Install the inside handle bezel.
4. Install the inside handle bezel screw.

Tighten
Tighten the inside handle bezel screw to 1.4 N·m (12 lb in).

5. Install the door switch panel to the door.
6. Connect the switches electrical connectors.