For 1990-2009 cars

## Fog Lamps Always On Domestic

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire Fog Lights System Check performed? | -- | Go to Step 2 | Go to Fog Lights System Check
2 |

1. Place the fog lamp switch in the OFF position.
2. Disconnect the foglamp relay located in the underhood electrical center.

Do the fog lamps turn off?

--

Go to Step 3

Go to Step 4

3 | With a test light to ground, probe the foglamp relay cavity F11 in the underhood electrical center. Does the test light illuminate? | -- | Go to Step 5 | Go to Step 6
4 | Repair the short to B+ in circuit 34 between the fog lamps and the foglamp relay. Is the repair complete? | -- | Go to Step 9 | --
5 |

1. Disconnect the connector from the fog lamp switch.
2. With a test light to ground, probe the fog lamp relay cavity F11 in the underhood electrical center.

Does the test light illuminate?

--

Go to Step 7

Go to Step 8

6 | Replace the foglamp relay. Refer to Fog Lamp Relay Replacement Is the repair complete? | -- | Go to Step 9 | --
7 | Repair the short to B+ in circuit 317 between the fog lamp switch and the fog lamp relay. Is the repair complete? | -- | Go to Step 9 | --
8 | Replace the fog lamp switch. Refer to Fog Lamp Switch Replacement . Is the repair complete? | -- | Go to Step 9 | --
9 |

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors/components removed.

Have all repairs been made?

--

Go to Fog Lights System Check

--

## Fog Lamps Always On Europe

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire Fog Lights System Check performed? | -- | Go to Step 2 | Go to Fog Lights System Check
2 | Repair the short to B+ in circuit 122. Is the repair complete? | -- | Go to Step 3 | --
3 |

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors/components removed.

Have all the repairs been made?

--

Go to Fog Lights System Check

--