For 1990-2009 cars

# SMU-SEC. 8A-40-REV. DIAGNOSTIC CHART 1 (HORNS INOP. FROM SWIT

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 8A-40 - REVISED DIAGNOSTIC CHART #1 (HORNS INOPERATIVE FROM SWITCH(ES))

#### MODELS: 1998 CHEVROLET CAMARO 1998 PONTIAC FIREBIRD

THIS BULLETIN IS BEING ISSUED TO REVISE DIAGNOSTIC CHART #1 (HORNS INOPERATIVE FROM SWITCH(ES)) ON PAGE 8A-40-2 OF THE SERVICE MANUAL (GMP/98-F-1).

PLEASE REPLACE THE CURRENT CHART #1 WITH THE ATTACHED.

FIGURES: 00 ATTACHMENTS: 01

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.