For 1990-2009 cars

### Removal Procedure

1. Remove the lock rod knob (3) from the lock rod (2).
2. Pull the door inside handle open to access the bezel screws.
3. On Pontiac, remove the inside handle bezel screw.
4. On Chevrolet , remove the switch plate panel.
5. On Chevrolet, remove the inside handle bezel screws.
6. Unsnap the bezel from the door trim panel.
7. Disconnect the light bulb from the rear of the bezel.
8. Remove the inside door handle bezel from the vehicle.

### Installation Procedure

1. Install the inside door handle bezel to the vehicle.
2. Connect the light bulb to the rear of the bezel.
3. Snap the bezel to the door trim panel.
4. On Chevrolet, install the inside handle bezel screws.

Tighten
Tighten the inside handle bezel screws to 1.4 N·m (12 lb in).

5. On Chevrolet, install the switch plate panel.
6. On Pontiac, install the inside door handle bezel screw.

Tighten
Tighten the inside handle bezel screws to 1.4 N·m (12 lb in).

7. Install the lock rod knob (3), perform the following:

7.1. | Pull the lock rod (2) forward in pocket or inside the bezel.

7.2. | Align the lock rod knob (3) over the lock rod (2).

7.3. | Insert rearward end of lock rod knob (3) through the hole inside the bezel.

7.4. | Pull the knob (3) rearward until the end of the rod (2) slides into the depression end of the knob (3).

7.5. | Apply pressure to snap knob (3) over lock rod (2).