For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the battery negative cable.
2. Remove the instrument panel driver knee bolster. Refer to Instrument Panel, Gauges and Console.
3. Remove the electrical connector from the clutch pedal position switch.
4. Remove the clutch pedal position switch from the brake and accelerator and clutch pedal with the bracket.

### Installation Procedure

1. Install the clutch pedal position switch to the brake and accelerator and clutch pedal with the bracket.
2. Install the electrical connector to the clutch pedal position switch.
3. Install the instrument panel driver knee bolster. Refer to Instrument Panel, Gauge and Console section in General Information.
4. Connect the battery negative cable.