For 1990-2009 cars

## Compressor Clutch Plate and Hub Assembly Removal V5 - Conventional Mount

#### Tools Required

• | J 33022 6-Point 13 mm Socket

• | J 33027-A Clutch Hub Holding Tool

• | J 33013-B Hub And Drive Plate Remover/Installer

• | J 34992 Compressor Holding Fixture

1. Clamp the J 34992 in a vise.
2. Attach the A/C compressor to the holding fixture using the thumb screws.
3. Use the J 33027-A in order to prevent the clutch hub and drive plate assembly from turning.
4. Use the J 33022 in order to remove the shaft nut.
5. Thread the J 33013-B into the hub.
6. Use a wrench in order to hold the body of the J 33013-B .
7. Turn the center screw into the body of the J 33013-B in order to remove the clutch plate and hub assembly.
8. Remove the shaft key. Retain the shaft key for reassembly.

## Compressor Clutch Plate and Hub Assembly Removal V7 - Direct Mount

#### Tools Required

• | J 33013-B Hub and Drive Plate Remover/Installer

• | J 33027-A Clutch Hub Holding Tool

• | J 41790-A A/C Compressor Holding Fixture

1. Remove the A/C compressor from the vehicle.
2. Clamp the A/C compressor holding fixture, J 41790-A in a vise and attach the A/C compressor to the J 41790-A .
3. Hold the clutch hub and drive plate assembly (2) in place using the J 33027-A .
4. Remove the A/C compressor shaft nut with a 13 mm socket (1).
5. Thread the J 33013-B into the hub.
6. Remove the hub and drive plate assembly (1) by turning the center screw into the body of the J 33013-B and against the A/C compressor shaft.
7. Remove the shaft key and retain for reassembly.